**Fixing plate**

For Ø 20mm tubes

Reference: **2392**

Specification description

Pack of two fixing plates for Ø 20mm shower curtain rails.

To mount shower curtain rail assembly.

Concealed fixings via a 304 stainless steel fixing plate.

With push-fit connectors for mounting.

Supplied with 4 screws 4 x 30 and 4 rawl plugs.

30-year warranty.