**TEMPOSTOP time flow tap**

Wall-mounted, M½"

Reference: **746410**

Specification description

Wall-mounted lever-operated time flow tap:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant tamperproof flow straightener.

Chrome-plated brass M½".

Lever-operated (soft-touch operation).

30-year warranty.