**MIXFOOT instant mixer**

Pedal-operated

Wall-mounted

Reference: **739102**

Specification description

Foot-operated basin mixer with instant flow:

Instant automatic shut-off.

Pedal can be raised for cleaning the floor.

Adjustable pedal height.

Fixing with 4 screws.

Filters.

Pre-set mixing can be adjusted: half open for cold water and fully open for mixed water (pedal against floor).

Wall-mounted M½".

30-year warranty.