**TEMPOSTOP time flow shower kit**

Time flow

Exposed, with chain-pull, fixed head GYM

Reference: **747006**

Specification description

Ceiling mounted chain-pull time flow shower kit:

TEMPOSTOP M½" time flow valve for mixed water, top supply.

For ceiling-mounting.

Time flow ~15 seconds.

Flow rate 6 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass body.

Lever and chain fitted with handle.

With fixed, scale-resistant and tamperproof shower head GYM.

30-year warranty.