**Flow rate regulators**

10 lpm ± 10 %

Reference: **927015.5P**

Specification description

Flow rate regulator.

FM1/2".

Recommended for automatic bath/shower reversers.

Creates a backpressure that maintains the shower position in case of low pressure.

10 lpm at 3 bar ± 10 %.

Supplied in packs of 5 pieces.

30-year warranty.