**Shower head**

With grid

Wall-mounted

Reference: **64000**

Specification description

Wall-mounted shower head with grid.

Compact, fixed and tamperproof shower head.

5 ring spray plate.

Grub screw fixing.

40 lpm at 3 bar without flow limiter.

For recessed water inlet.

30-year warranty.