**Deck-mounted single hole mixer - 45 lpm**

Swivelling over spout L. 300mm H. 290mm

Reference: **G66453**

Specification description

Deck-mounted single hole mixer for professional kitchens.

Mixer for plunge sinks with swivelling, tubular spout H. 290mm L. 300mm.

Star-shaped flow straightener with smooth interior.

Water-free valve heads with control knobs.

Flow rate 45 lpm at 3 bar.

Chrome-plated brass body and spout.

F3/8" PEX flexibles.

Mixer suitable for intensive use in professional kitchens.

Single hole tap

30-year warranty.