**Safety shower head**

Reference: **9225**

Specification description

Round safety shower head, Ø 250mm M1" in green, shock-resistant ABS.

Flow rate 132 lpm at 3 bar dynamic pressure).

Water supply F1".

30-year warranty