**Scale-resistant aerator**

M24/100

20 to 25 lpm, pack of 5

Reference: **24.5P**

Specification description

Scale-resistant aerator without limiter.

M24/100.

Flow rate 20 to 25 lpm at 3 bar.

Delivered in packs of 5.