**Pre-rinse set with mixer**

Without bib tap

White flexible and scale-resistant hand spray

Reference: **G6633**

Specification description

Complete pre-rinse set without bib tap.

suitable for intensive use in professional kitchens.

Single hole deck-mounted mixer with:

- valve head with control knobs.

- F3/8" connectors and non-return valves.

- reinforced fixing via 2 threaded rods and back-nuts.

White hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433000).

Scale-resistant hand spray and shock-resistant tip.

White, reinforced, food-grade flexible hose L. 0.95m.

3/4" stainless steel column.

Adjustable wall bracket.

Stainless steel spring guide.

Pre-rinse set

30-year warranty.