**Pre-rinse set with mixer**

Without bib tap

Black flexible and scale-resistant hand spray

Reference: **5630**

Specification description

Complete pre-rinse set without bib tap suitable for intensive use in professional kitchens.

Deck-mounted single hole mixer with:

- valve heads with reinforced mechanisms and ergonomic control levers.

- F3/8" flexibles and non-return valves.

- reinforced fixing via 2 threaded rods with back-nuts.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray with shock-resistant tip.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" stainless steel column.

Adjustable wall bracket.

Stainless steel spring guide.

Pre-rinse set with 30-year warranty.