**White powder-coated stainless steel coat hook**

White powder-coated 304 stainless steel

Reference: **4042W**

Specification description

Double coat hook.

Wall-mounted coat hook.

Bacteriostatic white powder-coated 304 stainless steel

Concealed fixings.

Tube Ø 20mm, 1mm thick.

Dimensions: Ø 62 x 55 x 95mm.

30-year warranty.