**AQUEDUTO wall-mounted washbasin**

Polished satin 304 stainless steel - concealed drainage

Without tap hole

Reference: **120150**

Specification description

Wall-mounted washbasin, 700x440mm.

Sleek and timeless design.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm

Rounded edges prevent injury.

With no tap hole.

Supplied with 1¼" waste.

Without overflow.

Supplied with brackets and fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 12kg.

30-year warranty.

[Formerly ref: 0211150015]