**Floor-standing XL P disposal sink**

Polished satin 304 stainless steel - top inlet

Reference: **182070**

Specification description

Floor-standing disposal sink.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

Smooth surface is easy to clean.

Concealed perimetral flushing system.

Horizontal or vertical water inlet: Ø 55mm.

Horizontal or vertical water outlet: Ø 100mm.

Supplied with PVC pipe.

Concealed drainage: shrouded sink.

Quick and easy to install: 2 access panels

with theft prevention TORX security screws.

Hinged stainless steel bucket grid.

Weight: 16kg.

30-year warranty.

[Formerly ref: 0710200007]