**Wall-mounted XL S disposal sink**

Polished satin 304 stainless steel - rear inlet

Reference: **182160**

Specification description

Wall-mounted disposal sink.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm

Smooth surface for easy cleaning.

Concealed perimetral flushing system.

Horizontal water inlet: Ø 55mm.

Recessed horizontal waste outlet: Ø 100mm.

Concealed drainage: shrouded sink.

Quick and easy to install from the front thanksto a stainless steel mounting frame.

Hinged stainless steel bucket grid.

Weight: 15kg.

30-year warranty.

[Formerly ref: 0711210006]