**Twin toilet roll holder**

For toilet rolls

Bright polished 304 stainless steel

Reference: **510082P**

Specification description

Wall-mounted toilet roll holder.

Twin toilet roll holder.

Bacteriostatic bright polished 304 stainless steel.

Tube Ø 20mm, 1mm thick.

Concealed fixings.

30-year warranty.