**Surgical scrub-up trough with high upstand**

Polished satin 304 stainless steel - 1 service - "Hygiene+" Design

With 1 single tap hole Ø 22mm per service

Reference: **185100**

Specification description

Wall-mounted surgical scrub-up trough with 450mm upstand.

Suitable for hospitals and healthcare facilities.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

Length 700mm, 1 service. With 1 tap hole Ø 22mm.

Smooth surface and rounded inside edges for easy cleaning.

"Hygiene+" design: reduces niches where bacteria can develop, concealed trap, easy to clean.

Drainage on the right. Without overflow. Supplied with fixing elements.

CE marked. Complies with norm EN 14296.

Weight: 20.3kg

30-year warranty.