**BINOPTIC wall-mounted electronic soap dispenser**

Electronic liquid or foam soap, or hydroalcoholic gel dispenser

Mains, chrome-plated 304 stainless steel, 1L tank

Reference: **512051P**

Specification description

Wall-mounted electronic soap dispenser.

Liquid or foam soap or hydroalcoholic gel dispenser.

No manual contact: infrared cell detects hands automatically.

Chrome-plated 304 stainless steel spout.

No waste pump dispenser.

Independent electronic housing and removable tank enable installation beneath the washbasin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Compatible with hydroalcoholic gel

Total spout length: 115mm.

Supplied with 1-litre tank.

Wall-mounted electronic soap dispenser with 30-year warranty.

CE marked.