**Flexible hose for auto-rewind hose reel**

L. 15m

Reference: **435576**

Specification description

Flexible hose L. 15m for auto-rewind hose reels 5675T2 and 5676T2.

Maximum temperature: 70°C.

Maximum pressure: 20 bar constant.