**Twin hole pre-rinse set with mixer**

Without bib tap

Black flexible and scale-resistant hand spray

Reference: **5880**

Specification description

Complete pre-rinse set without bib tap suitable for intensive use in professional kitchens.

Deck-mounted twin hole mixer, 150mm centres, with:

- valve heads with reinforced mechanisms and ergonomic controls.

- offset inlet connections with M1/2" tails.

Black hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433009).

Scale-resistant hand spray with shock-resistant tip.

Black, reinforced food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

These pre-rinse sets can be installed close to the splashback.