**BINOPTIC deck-mounted electronic soap dispenser**

Liquid or foam soap dispenser

Mains, matte black 304 stainless steel, 1.2m tube

Reference: **512121BK**

Specification description

Deck--mounted electronic soap dispenser.

Liquid or foam soap dispenser.

No manual contact: infrared cell detects hands automatically.

Matte black 304 stainless steel spout.

No waste pump dispenser.

Separate electronic unit for installation beneath the washbasin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Spout length: 105mm.

Supplied with 1.20m flexible tube for remote tanks (tank not supplied).

Deck-mounted electronic soap dispenser.

30-year warranty.

CE marked.