**RAINY shower head**

Rain-effect shower head

Scale-resistant

Reference: **708040**

Specification description

Shower head.

Flow rate 6 lpm at 3 bar.

A higher flow rate can be achieved: remove flow rate regulator.

Scale-resistant head with nozzles.

Soft rain-effect flow engulfs user.

Chrome-plated metal.

Inlet M½".

Available for ceiling or wall-mounted installation.

Depending on installation: can be fitted with a horizontal shower arm (ref: 710040) or a vertical shower arm (ref: 710050).

30-year warranty.