**Solenoid valve**

For TEMPOMATIC 3 urinals

Ø28mm - 6V

Reference: **492647**

Specification description

Solenoid valve.

For TEMPOMATIC 3 urinals.

Unions M Ø11mm.

Works with a 6V power supply.

Dimensions: 39mm, Ø 28,5mm, cable: 100mm.