**Reinforced exposed union**

For TEMPOMATIC 3 4

Reference: **841215**

Specification description

Reinforced exposed union.

Supplied with sleek concealment plate.

Recommended for the installation of TEMPOMATIC 3 (443006) or TEMPOMATIC 4 (443436, 443536) wall-mounted basin taps with exposed supply.

30-year warranty.