**Electronic control unit**

For TEMPOMATIC 4

Battery-operated

Reference: **490446**

Specification description

Electronic control unit.

For TEMPOMATIC 4.

Works with 6V batteries (included).

Dimensions: 67mm, Ø 51mm.