**Solenoid valve**

For TEMPOMATIC WCs and urinals

MM1" - 12V

Reference: **461035**

Specification description

Solenoid valve.

For TEMPOMATIC WCs and urinals.

Unions MM1".

Works with a 12V power supply.

Dimensions: 108 x 107mm.