**BINOPTIC wall-mounted electronic soap dispenser**

Liquid or foam soap or hydroalcoholic gel dispenser

Mains supply, satin 304 stainless steel,1L tank

Reference: **512051S**

Specification description

Wall-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Spout made from satin finish 304 stainless steel.

No-waste pump dispenser.

Separate electronic unit and removable tank for installation under the basin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specialist foam soap.

Compatible with hydroalcoholic gel.

Total spout length: 115mm.

Supplied with a 1 litre tank.

 Wall-mounted electronic soap dispenser with 30-year warranty.

CE marked.