**Soleinoid valve**

For shower and urinal

MM1/2", 6V, with filter

Reference: **495615**

Specification description

Solenoid valve with filter.

For product range TEMPOMATIC urinal and SECURITHERM shower.

M1/2" connectors.

Dimensions: 64 x 50mm.