**2-function unit for installation behind a mirror**

Hand dryer and soap dispenser

To be fitted behind mirror cabinet, mains supply

Reference: **510207I**

Specification description

2-function unit: electronic soap dispenser and air pulse hand dryer.

• Quick and easy to install in a cabinet or behind a mirror.

• Fixings at the back and sides.

• 304 stainless steel support, 1.2 mm thick.

• Supplied with self-adhesive pictograms to indicate the location of the different functions on the mirror/cabinet: soap and air.

• Vandal-resistant model with standard DELABIE key.

• 30-year warranty (3-year warranty for the hand dryer).

• CE marked.