35082W

**Basic angled grab bar 135°, white, 400 x 400mm**

Reference: 35082W

Specification Description

Basic angled grab bar 135°, Ø 32mm, for people with reduced mobility.

White powder-coated stainless steel tube.

3 fixing points prevent the hand from getting trapped and simplify installation.

Dimensions: 400 x 400mm.

 Fixings concealed by 3-hole stainless steel plate.

 CE marked.

10-year warranty.