510583

**Wall-mounted liquid soap dispenser, 0.5 litres**

Reference: 510583

Specification Description

Wall-mounted liquid soap dispenser with soft-touch operation.

Vandal-resistant model with lock and standard DELABIE key.

One piece hinged cover for easy maintenance and improved hygiene.

Soft-touch push button.

Anti-blocking: one dose per push even if button is held in place.

No waste, non-drip (waterproof) pump dispenser.

Tank prevents the long-term stagnation of soap.

Tank with large opening: eases transfer of soap from large containers.

Window for monitoring soap level.

Bright polished 304 stainless steel.

Stainless steel thickness: 1 mm.

Capacity: 0.5 litres.

Dimensions: 90 x 105 x 185mm.

For vegetable based liquid soap with a maximum viscosity: 3,000 mPa.s.

Compatible with hydroalcoholic gel.

10-year warranty.