DELABIE_C100M35729150

**Liquid soap dispenser**

Reference: 729150

Specification Description

Wall-mounted liquid soap dispenser for cross wall installation for walls up to 180mm.

For remote tanks (tank not supplied).

Chrome-plated brass body and push-button, with flexible pipe 6/8, L. 1.20m.

Non-drip system (waterproof).

Mechanism can be locked via grub screw.

For remote tanks (tank not supplied) supplied with a 1.2m rilsan tube for remote tanks.

10-year warranty.